**DJ-VX50 Firmware upgrade Instructions.**



1. Install
2. Run “DJ-VX50HT Upgrade” in “Administrator mode”



* *(Place the Mouse curser on “DJ-VX50HT Upgrade” icon and Right click the Mouse button)*

*Select “****Properties****” and click on “****Compatibility****” Check on “****Run this program as an Administrator****”*

1. Plug in the Alinco USB Data Cable ERW-7 or ERW-15 to your PC and radio. *(Make sure to check the “COM Port” Number assigned to the cable in your PC’s Device manager settings). Power on the radio.*
2. Run “DJ-VX50THT Upgrade” Select COM Port assigned to the Data cables
3. If you get an error “**MSCOMM32.OCX**”, please copy this file included with the firmware

to your PC “C:/Program Files/DJ-VX50HT Upgrade” folder and run the program again.

1. Select “Upgrade” and this should initiate the Upgrade process.



1. Check the firmware version

* Press FUNC then press and hold "#"key until radio keypad is locked.
* Press the "ESC" key 5 times. The LCD will display the version is 1.23

1. Remember to unlock the keypad after finish (press FUNC then press and hold "#"key to unlock keypad
2. You must factory “reset” after firmware update is performed

- Press and hold “PF2” key + PTT key and turn on the Radios

- Let go of the keys. You will see “DSP” Freq.

- Press arrow “Up” Key and you will see ”RESET”

- Turn the main dial knob to “FACT” and hit “FUNC” key

- Enter “000000” (6 digits) and the unit will perform RESET

© 2020 REMTronix Inc. eMail: [support@remtronix.com](mailto:support@remtronix.com). All Rights Reserved